---
title: "arduino - translation progress for f30"
package: arduino
date: 2025-12-13T17:27:21.304359+00:00
started_languages: 62
no_languages: 0
polib_error_count: 0
could_not_process_count: 0
release: f30
---
The package arduino:

* represents 6186 source words to be translated
* is translated into 63 languages in Fedora f30




| Language | Translated words | Total source words | Progress (%) | Files |
|----------|-----------------:|-------------------:|-------------:|-------|
 | [bg]({{< ref "/f30/language/bg.md" >}}) | 3093 | 3093 | 100.0 | /mnt/stockage/packages/f30/arduino/arduino-core/src/processing/app/i18n/Resources_bg.po | 
 | [cs]({{< ref "/f30/language/cs.md" >}}) | 3093 | 3093 | 100.0 | /mnt/stockage/packages/f30/arduino/arduino-core/src/processing/app/i18n/Resources_cs_CZ.po | 
 | [en]({{< ref "/f30/language/en.md" >}}) | 3093 | 3093 | 100.0 | /mnt/stockage/packages/f30/arduino/arduino-core/src/processing/app/i18n/Resources_en.po | 
 | [hu]({{< ref "/f30/language/hu.md" >}}) | 3093 | 3093 | 100.0 | /mnt/stockage/packages/f30/arduino/arduino-core/src/processing/app/i18n/Resources_hu.po | 
 | [it]({{< ref "/f30/language/it.md" >}}) | 3093 | 3093 | 100.0 | /mnt/stockage/packages/f30/arduino/arduino-core/src/processing/app/i18n/Resources_it_IT.po | 
 | [ja]({{< ref "/f30/language/ja.md" >}}) | 3093 | 3093 | 100.0 | /mnt/stockage/packages/f30/arduino/arduino-core/src/processing/app/i18n/Resources_ja_JP.po | 
 | [ko]({{< ref "/f30/language/ko.md" >}}) | 3093 | 3093 | 100.0 | /mnt/stockage/packages/f30/arduino/arduino-core/src/processing/app/i18n/Resources_ko_KR.po | 
 | [pl]({{< ref "/f30/language/pl.md" >}}) | 3093 | 3093 | 100.0 | /mnt/stockage/packages/f30/arduino/arduino-core/src/processing/app/i18n/Resources_pl.po | 
 | [ru]({{< ref "/f30/language/ru.md" >}}) | 3093 | 3093 | 100.0 | /mnt/stockage/packages/f30/arduino/arduino-core/src/processing/app/i18n/Resources_ru.po | 
 | [sk]({{< ref "/f30/language/sk.md" >}}) | 3093 | 3093 | 100.0 | /mnt/stockage/packages/f30/arduino/arduino-core/src/processing/app/i18n/Resources_sk.po | 
 | [uk]({{< ref "/f30/language/uk.md" >}}) | 3093 | 3093 | 100.0 | /mnt/stockage/packages/f30/arduino/arduino-core/src/processing/app/i18n/Resources_uk.po | 
 | [es]({{< ref "/f30/language/es.md" >}}) | 3091 | 3093 | 99.9 | /mnt/stockage/packages/f30/arduino/arduino-core/src/processing/app/i18n/Resources_es.po | 
 | [de]({{< ref "/f30/language/de.md" >}}) | 3089 | 3093 | 99.9 | /mnt/stockage/packages/f30/arduino/arduino-core/src/processing/app/i18n/Resources_de_DE.po | 
 | [fr]({{< ref "/f30/language/fr.md" >}}) | 3089 | 3093 | 99.9 | /mnt/stockage/packages/f30/arduino/arduino-core/src/processing/app/i18n/Resources_fr.po | 
 | [pt_BR]({{< ref "/f30/language/pt_BR.md" >}}) | 3089 | 3093 | 99.9 | /mnt/stockage/packages/f30/arduino/arduino-core/src/processing/app/i18n/Resources_pt_BR.po | 
 | [en_GB]({{< ref "/f30/language/en_GB.md" >}}) | 3049 | 3093 | 98.6 | /mnt/stockage/packages/f30/arduino/arduino-core/src/processing/app/i18n/Resources_en_GB.po | 
 | [et]({{< ref "/f30/language/et.md" >}}) | 6090 | 6186 | 98.4 | /mnt/stockage/packages/f30/arduino/arduino-core/src/processing/app/i18n/Resources_et_EE.po/mnt/stockage/packages/f30/arduino/arduino-core/src/processing/app/i18n/Resources_et.po | 
 | [pt_PT]({{< ref "/f30/language/pt_PT.md" >}}) | 2973 | 3093 | 96.1 | /mnt/stockage/packages/f30/arduino/arduino-core/src/processing/app/i18n/Resources_pt_PT.po | 
 | [zh_Hans]({{< ref "/f30/language/zh_Hans.md" >}}) | 2972 | 3093 | 96.1 | /mnt/stockage/packages/f30/arduino/arduino-core/src/processing/app/i18n/Resources_zh_CN.po | 
 | [ca]({{< ref "/f30/language/ca.md" >}}) | 2969 | 3093 | 96.0 | /mnt/stockage/packages/f30/arduino/arduino-core/src/processing/app/i18n/Resources_ca.po | 
 | [el]({{< ref "/f30/language/el.md" >}}) | 2925 | 3093 | 94.6 | /mnt/stockage/packages/f30/arduino/arduino-core/src/processing/app/i18n/Resources_el_GR.po | 
 | [zh_Hant]({{< ref "/f30/language/zh_Hant.md" >}}) | 2884 | 3093 | 93.2 | /mnt/stockage/packages/f30/arduino/arduino-core/src/processing/app/i18n/Resources_zh_TW.po | 
 | [ro]({{< ref "/f30/language/ro.md" >}}) | 2830 | 3093 | 91.5 | /mnt/stockage/packages/f30/arduino/arduino-core/src/processing/app/i18n/Resources_ro.po | 
 | [ar]({{< ref "/f30/language/ar.md" >}}) | 2798 | 3093 | 90.5 | /mnt/stockage/packages/f30/arduino/arduino-core/src/processing/app/i18n/Resources_ar.po | 
 | [tr]({{< ref "/f30/language/tr.md" >}}) | 2789 | 3093 | 90.2 | /mnt/stockage/packages/f30/arduino/arduino-core/src/processing/app/i18n/Resources_tr.po | 
 | [hy]({{< ref "/f30/language/hy.md" >}}) | 2748 | 3093 | 88.8 | /mnt/stockage/packages/f30/arduino/arduino-core/src/processing/app/i18n/Resources_hy.po | 
 | [nb_NO]({{< ref "/f30/language/nb_NO.md" >}}) | 2698 | 3093 | 87.2 | /mnt/stockage/packages/f30/arduino/arduino-core/src/processing/app/i18n/Resources_nb_NO.po | 
 | [be]({{< ref "/f30/language/be.md" >}}) | 2334 | 3093 | 75.5 | /mnt/stockage/packages/f30/arduino/arduino-core/src/processing/app/i18n/Resources_be.po | 
 | [vi]({{< ref "/f30/language/vi.md" >}}) | 2317 | 3093 | 74.9 | /mnt/stockage/packages/f30/arduino/arduino-core/src/processing/app/i18n/Resources_vi.po | 
 | [ka]({{< ref "/f30/language/ka.md" >}}) | 2209 | 3093 | 71.4 | /mnt/stockage/packages/f30/arduino/arduino-core/src/processing/app/i18n/Resources_ka_GE.po | 
 | [pt]({{< ref "/f30/language/pt.md" >}}) | 2046 | 3093 | 66.1 | /mnt/stockage/packages/f30/arduino/arduino-core/src/processing/app/i18n/Resources_pt.po | 
 | [he]({{< ref "/f30/language/he.md" >}}) | 1983 | 3093 | 64.1 | /mnt/stockage/packages/f30/arduino/arduino-core/src/processing/app/i18n/Resources_iw.po | 
 | [gl]({{< ref "/f30/language/gl.md" >}}) | 3764 | 6186 | 60.8 | /mnt/stockage/packages/f30/arduino/arduino-core/src/processing/app/i18n/Resources_gl_ES.po/mnt/stockage/packages/f30/arduino/arduino-core/src/processing/app/i18n/Resources_gl.po | 
 | [eu]({{< ref "/f30/language/eu.md" >}}) | 1879 | 3093 | 60.8 | /mnt/stockage/packages/f30/arduino/arduino-core/src/processing/app/i18n/Resources_eu.po | 
 | [an]({{< ref "/f30/language/an.md" >}}) | 1868 | 3093 | 60.4 | /mnt/stockage/packages/f30/arduino/arduino-core/src/processing/app/i18n/Resources_an.po | 
 | [hr]({{< ref "/f30/language/hr.md" >}}) | 1854 | 3093 | 59.9 | /mnt/stockage/packages/f30/arduino/arduino-core/src/processing/app/i18n/Resources_hr_HR.po | 
 | [sq]({{< ref "/f30/language/sq.md" >}}) | 1854 | 3093 | 59.9 | /mnt/stockage/packages/f30/arduino/arduino-core/src/processing/app/i18n/Resources_sq.po | 
 | [fi]({{< ref "/f30/language/fi.md" >}}) | 1843 | 3093 | 59.6 | /mnt/stockage/packages/f30/arduino/arduino-core/src/processing/app/i18n/Resources_fi.po | 
 | [nl]({{< ref "/f30/language/nl.md" >}}) | 3468 | 6186 | 56.1 | /mnt/stockage/packages/f30/arduino/arduino-core/src/processing/app/i18n/Resources_nl_NL.po/mnt/stockage/packages/f30/arduino/arduino-core/src/processing/app/i18n/Resources_nl.po | 
 | [sl]({{< ref "/f30/language/sl.md" >}}) | 1676 | 3093 | 54.2 | /mnt/stockage/packages/f30/arduino/arduino-core/src/processing/app/i18n/Resources_sl_SI.po | 
 | [sv]({{< ref "/f30/language/sv.md" >}}) | 1675 | 3093 | 54.2 | /mnt/stockage/packages/f30/arduino/arduino-core/src/processing/app/i18n/Resources_sv.po | 
 | [lv]({{< ref "/f30/language/lv.md" >}}) | 1656 | 3093 | 53.5 | /mnt/stockage/packages/f30/arduino/arduino-core/src/processing/app/i18n/Resources_lv_LV.po | 
 | [error]({{< ref "/f30/language/error.md" >}}) | 1560 | 3093 | 50.4 | /mnt/stockage/packages/f30/arduino/arduino-core/src/processing/app/i18n/Resources_zh_TW.Big5.po | 
 | [fr_CA]({{< ref "/f30/language/fr_CA.md" >}}) | 1444 | 3093 | 46.7 | /mnt/stockage/packages/f30/arduino/arduino-core/src/processing/app/i18n/Resources_fr_CA.po | 
 | [id]({{< ref "/f30/language/id.md" >}}) | 1401 | 3093 | 45.3 | /mnt/stockage/packages/f30/arduino/arduino-core/src/processing/app/i18n/Resources_in.po | 
 | [hi]({{< ref "/f30/language/hi.md" >}}) | 1322 | 3093 | 42.7 | /mnt/stockage/packages/f30/arduino/arduino-core/src/processing/app/i18n/Resources_hi.po | 
 | [ta]({{< ref "/f30/language/ta.md" >}}) | 1309 | 3093 | 42.3 | /mnt/stockage/packages/f30/arduino/arduino-core/src/processing/app/i18n/Resources_ta.po | 
 | [fil]({{< ref "/f30/language/fil.md" >}}) | 1259 | 3093 | 40.7 | /mnt/stockage/packages/f30/arduino/arduino-core/src/processing/app/i18n/Resources_fil.po | 
 | [fa]({{< ref "/f30/language/fa.md" >}}) | 2069 | 6186 | 33.4 | /mnt/stockage/packages/f30/arduino/arduino-core/src/processing/app/i18n/Resources_fa_IR.po/mnt/stockage/packages/f30/arduino/arduino-core/src/processing/app/i18n/Resources_fa.po | 
 | [da]({{< ref "/f30/language/da.md" >}}) | 206 | 3093 | 6.7 | /mnt/stockage/packages/f30/arduino/arduino-core/src/processing/app/i18n/Resources_da_DK.po | 
 | [ne]({{< ref "/f30/language/ne.md" >}}) | 203 | 3093 | 6.6 | /mnt/stockage/packages/f30/arduino/arduino-core/src/processing/app/i18n/Resources_ne.po | 
 | [mr]({{< ref "/f30/language/mr.md" >}}) | 199 | 3093 | 6.4 | /mnt/stockage/packages/f30/arduino/arduino-core/src/processing/app/i18n/Resources_mr.po | 
 | [fy]({{< ref "/f30/language/fy.md" >}}) | 183 | 3093 | 5.9 | /mnt/stockage/packages/f30/arduino/arduino-core/src/processing/app/i18n/Resources_fy.po | 
 | [bs]({{< ref "/f30/language/bs.md" >}}) | 174 | 3093 | 5.6 | /mnt/stockage/packages/f30/arduino/arduino-core/src/processing/app/i18n/Resources_bs.po | 
 | [tzl]({{< ref "/f30/language/tzl.md" >}}) | 131 | 3093 | 4.2 | /mnt/stockage/packages/f30/arduino/arduino-core/src/processing/app/i18n/Resources_tzl.po | 
 | [ast]({{< ref "/f30/language/ast.md" >}}) | 124 | 3093 | 4.0 | /mnt/stockage/packages/f30/arduino/arduino-core/src/processing/app/i18n/Resources_ast.po | 
 | [my]({{< ref "/f30/language/my.md" >}}) | 93 | 3093 | 3.0 | /mnt/stockage/packages/f30/arduino/arduino-core/src/processing/app/i18n/Resources_my_MM.po | 
 | [lt]({{< ref "/f30/language/lt.md" >}}) | 91 | 3093 | 2.9 | /mnt/stockage/packages/f30/arduino/arduino-core/src/processing/app/i18n/Resources_lt_LT.po | 
 | [af]({{< ref "/f30/language/af.md" >}}) | 12 | 3093 | 0.4 | /mnt/stockage/packages/f30/arduino/arduino-core/src/processing/app/i18n/Resources_af.po | 
 | [ach]({{< ref "/f30/language/ach.md" >}}) | 0 | 3093 | 0.0 | /mnt/stockage/packages/f30/arduino/arduino-core/src/processing/app/i18n/Resources_ach.po | 
 | [kk]({{< ref "/f30/language/kk.md" >}}) | 0 | 3093 | 0.0 | /mnt/stockage/packages/f30/arduino/arduino-core/src/processing/app/i18n/Resources_kk.po | 
 | [te]({{< ref "/f30/language/te.md" >}}) | 0 | 3093 | 0.0 | /mnt/stockage/packages/f30/arduino/arduino-core/src/processing/app/i18n/Resources_te.po | 
 | [th]({{< ref "/f30/language/th.md" >}}) | 0 | 3093 | 0.0 | /mnt/stockage/packages/f30/arduino/arduino-core/src/processing/app/i18n/Resources_th.po | 
{.sortable}

